No. Time Source Destination Protocol Length Info

1 0.000000 host 1.1.0 USB 48 GET DESCRIPTOR Request DEVICE

Frame 1: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x00

bDescriptorType: DEVICE (0x01)

Language Id: no language specified (0x0000)

wLength: 8

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

2 0.002439 1.1.0 host USB 48 GET DESCRIPTOR Response DEVICE

Frame 2: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

DEVICE DESCRIPTOR

bLength: 18

bDescriptorType: 0x01 (DEVICE)

bcdUSB: 0x0200

bDeviceClass: Device (0x00)

bDeviceSubClass: 0

bDeviceProtocol: 0 (Use class code info from Interface Descriptors)

bMaxPacketSize0: 64

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

3 0.002809 host 1.1.0 USB 48 GET DESCRIPTOR Request DEVICE

Frame 3: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x00

bDescriptorType: DEVICE (0x01)

Language Id: no language specified (0x0000)

wLength: 18

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

4 0.006422 1.1.0 host USB 58 GET DESCRIPTOR Response DEVICE

Frame 4: 58 bytes on wire (464 bits), 58 bytes captured (464 bits) on interface XHC1, id 0

USB URB

DEVICE DESCRIPTOR

bLength: 18

bDescriptorType: 0x01 (DEVICE)

bcdUSB: 0x0200

bDeviceClass: Device (0x00)

bDeviceSubClass: 0

bDeviceProtocol: 0 (Use class code info from Interface Descriptors)

bMaxPacketSize0: 64

idVendor: Inside Out Networks (0x0648)

idProduct: Unknown (0xeeee)

bcdDevice: 0xeeee

iManufacturer: 1

iProduct: 2

iSerialNumber: 3

bNumConfigurations: 1

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

5 0.006623 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 5: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x02

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 2

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

6 0.010427 1.1.0 host USB 42 GET DESCRIPTOR Response STRING

Frame 6: 42 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 32

bDescriptorType: 0x03 (STRING)

bString:

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

7 0.010478 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 7: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x02

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 32

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

8 0.014417 1.1.0 host USB 72 GET DESCRIPTOR Response STRING

Frame 8: 72 bytes on wire (576 bits), 72 bytes captured (576 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 32

bDescriptorType: 0x03 (STRING)

bString: STM32 USB 测试开发板

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

9 0.014514 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 9: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x01

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 2

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

10 0.018438 1.1.0 host USB 42 GET DESCRIPTOR Response STRING

Frame 10: 42 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 8

bDescriptorType: 0x03 (STRING)

bString:

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

11 0.018507 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 11: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x01

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 8

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

12 0.022420 1.1.0 host USB 48 GET DESCRIPTOR Response STRING

Frame 12: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 8

bDescriptorType: 0x03 (STRING)

bString: 欧大佬

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

13 0.022516 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 13: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x03

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 2

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

14 0.026419 1.1.0 host USB 42 GET DESCRIPTOR Response STRING

Frame 14: 42 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 28

bDescriptorType: 0x03 (STRING)

bString:

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

15 0.026458 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 15: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x03

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 28

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

16 0.030422 1.1.0 host USB 68 GET DESCRIPTOR Response STRING

Frame 16: 68 bytes on wire (544 bits), 68 bytes captured (544 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 28

bDescriptorType: 0x03 (STRING)

bString: USB2333333333

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

17 0.030532 host 1.1.0 USB 48 GET DESCRIPTOR Request CONFIGURATION

Frame 17: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x00

bDescriptorType: CONFIGURATION (0x02)

Language Id: no language specified (0x0000)

wLength: 9

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

18 0.034428 1.1.0 host USB 49 GET DESCRIPTOR Response CONFIGURATION

Frame 18: 49 bytes on wire (392 bits), 49 bytes captured (392 bits) on interface XHC1, id 0

USB URB

CONFIGURATION DESCRIPTOR

bLength: 9

bDescriptorType: 0x02 (CONFIGURATION)

wTotalLength: 32

bNumInterfaces: 1

bConfigurationValue: 1

iConfiguration: 4

Configuration bmAttributes: 0x80 NOT SELF-POWERED NO REMOTE-WAKEUP

bMaxPower: 200 (400mA)

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

19 0.034461 host 1.1.0 USB 48 GET DESCRIPTOR Request CONFIGURATION

Frame 19: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x00

bDescriptorType: CONFIGURATION (0x02)

Language Id: no language specified (0x0000)

wLength: 32

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

20 0.038418 1.1.0 host USB 72 GET DESCRIPTOR Response CONFIGURATION

Frame 20: 72 bytes on wire (576 bits), 72 bytes captured (576 bits) on interface XHC1, id 0

USB URB

CONFIGURATION DESCRIPTOR

bLength: 9

bDescriptorType: 0x02 (CONFIGURATION)

wTotalLength: 32

bNumInterfaces: 1

bConfigurationValue: 1

iConfiguration: 4

Configuration bmAttributes: 0x80 NOT SELF-POWERED NO REMOTE-WAKEUP

bMaxPower: 200 (400mA)

INTERFACE DESCRIPTOR (0.0): class Vendor Specific

bLength: 9

bDescriptorType: 0x04 (INTERFACE)

bInterfaceNumber: 0

bAlternateSetting: 0

bNumEndpoints: 2

bInterfaceClass: Vendor Specific (0xff)

bInterfaceSubClass: 0xff

bInterfaceProtocol: 0xff

iInterface: 5

ENDPOINT DESCRIPTOR

bLength: 7

bDescriptorType: 0x05 (ENDPOINT)

bEndpointAddress: 0x01 OUT Endpoint:1

bmAttributes: 0x02

wMaxPacketSize: 512

bInterval: 255

ENDPOINT DESCRIPTOR

bLength: 7

bDescriptorType: 0x05 (ENDPOINT)

bEndpointAddress: 0x81 IN Endpoint:1

bmAttributes: 0x02

wMaxPacketSize: 512

bInterval: 255

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

21 0.054906 host 1.1.0 USB 48 SET CONFIGURATION Request

Frame 21: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x00

bRequest: SET CONFIGURATION (9)

bConfigurationValue: 1

wIndex: 0 (0x0000)

wLength: 0

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

22 0.056476 1.1.0 host USB 40 SET CONFIGURATION Response

Frame 22: 40 bytes on wire (320 bits), 40 bytes captured (320 bits) on interface XHC1, id 0

USB URB

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

23 0.056630 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 23: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x05

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 2

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

24 0.060574 1.1.0 host USB 42 GET DESCRIPTOR Response STRING

Frame 24: 42 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 26

bDescriptorType: 0x03 (STRING)

bString:

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

25 0.060688 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 25: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x05

bDescriptorType: STRING (0x03)

Language Id: English (United States) (0x0409)

wLength: 26

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

26 0.064476 1.1.0 host USB 66 GET DESCRIPTOR Response STRING

Frame 26: 66 bytes on wire (528 bits), 66 bytes captured (528 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 26

bDescriptorType: 0x03 (STRING)

bString: 默认 Interface

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

27 0.094519 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 27: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x00

bDescriptorType: STRING (0x03)

Language Id: no language specified (0x0000)

wLength: 255

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

28 0.097466 1.1.0 host USB 44 GET DESCRIPTOR Response STRING

Frame 28: 44 bytes on wire (352 bits), 44 bytes captured (352 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 4

bDescriptorType: 0x03 (STRING)

wLANGID: Chinese (Macau SAR) (0x1404)

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

29 0.098513 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 29: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x01

bDescriptorType: STRING (0x03)

Language Id: Chinese (Macau SAR) (0x1404)

wLength: 255

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

30 0.098554 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 30: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x02

bDescriptorType: STRING (0x03)

Language Id: Chinese (Macau SAR) (0x1404)

wLength: 255

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

31 0.098574 host 1.1.0 USB 48 GET DESCRIPTOR Request STRING

Frame 31: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

Setup Data

bmRequestType: 0x80

bRequest: GET DESCRIPTOR (6)

Descriptor Index: 0x03

bDescriptorType: STRING (0x03)

Language Id: Chinese (Macau SAR) (0x1404)

wLength: 255

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

32 0.101456 1.1.0 host USB 48 GET DESCRIPTOR Response STRING

Frame 32: 48 bytes on wire (384 bits), 48 bytes captured (384 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 8

bDescriptorType: 0x03 (STRING)

bString: 欧大佬

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

33 0.105457 1.1.0 host USB 72 GET DESCRIPTOR Response STRING

Frame 33: 72 bytes on wire (576 bits), 72 bytes captured (576 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 32

bDescriptorType: 0x03 (STRING)

bString: STM32 USB 测试开发板

░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░░

No. Time Source Destination Protocol Length Info

34 0.109463 1.1.0 host USB 68 GET DESCRIPTOR Response STRING

Frame 34: 68 bytes on wire (544 bits), 68 bytes captured (544 bits) on interface XHC1, id 0

USB URB

STRING DESCRIPTOR

bLength: 28

bDescriptorType: 0x03 (STRING)

bString: USB2333333333